**READ BEFORE UPGRADING AP/CPE TO TR**

V01

# Example.

To update the equipment to the latest version in its TR mode, it must be accessed with the normal process indicated in the user manual of the product itself.

Next, access the menu to update the equipment itself and follow these steps:

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

1. Click ON **MANAGE.**
2. Then click **UPGRADE.**
3. Click select file and search and select upgrade file.
4. **IMPORTANT:** Always enable the "Restore to factory settings" check to perform a clean system reboot with the new version.
5. Finally click **UPGRADE** and wait.

Once the process is finished, we must configure it according to the user manual and according to the equipment to which we have updated:

* TR750: [TR 750 - Ekselans by ITS](https://www.ek.plus/en/product/tr-750/)
* TR1200: [TR 1200 - Ekselans by ITS](https://www.ek.plus/en/product/tr-1200/)
* TR1200OLP: [TR 1200 OLP - Ekselans by ITS](https://www.ek.plus/en/product/tr-1200-olp/)

For any questions about **Firmware** you can contact at [**soporte@ek.plus**](mailto:soporte@ek.plus) **.**

**Password to unzip FIRMWARE: leidomanualek.**