SETUP 780 (26/08/19)
--------------------
DTVIPI(S27H2F14) : Fix 16 services input limitation in multicast

SETUP 779 (26/07/09)
--------------------
EFHD4(H2) : H264 firmware (Hardware #2) upgrade V34 - bluray : detection of interlaced resolutions + HDCP power off/on problems fixed

SETUP 778 (26/07/02)
--------------------
EFHD4(H2) : H264 firmware (Hardware #2) downgrade to V26 - bluray : detection problem of interlaced resolutions 

SETUP 777 (26/06/08)
--------------------
DTVIFACE(v389) : add backplane mirroring option for RM98 (require RM98S96HxF12 - firmware update provided later)

SETUP 776 (26/06/03)
--------------------
DTVIFACE(v388) : fix DTVPCU configuration load erasing calibration/max current sensing value

SETUP 775 (26/05/28)
--------------------
RR13(ITEV12) : H264 encoder firmware fix no sound

SETUP 774 (26/05/26)
--------------------
RMIP(H1V60) : add no activity watchdog : fix FPGA demux random startup freeze

SETUP 773 (26/04/29)
--------------------
RM82(H3V31) : fix LEM diseqc switch problem : 22KHz now generated by LNBH26 (22KHz from STi not accurate : LNBH26 -> voltage dropout during diseqc message)
RM98(H1v95) : see above
RMIP(H1V59) : see above
RR12(H3V55) : see above

SETUP 772 (26/04/20)
--------------------
RR12(HxV54) : fix USB TS File read problem - H264 encoder firmware upgraded to V11 + H264 encoder logs capability added 

SETUP 771 (26/04/20)
--------------------
DTVIFACE(v387) : manufacturer mode : current limit setting added to calibration value

SETUP 770 (26/04/15)
--------------------
DTVIFACE(v386) : RM82 - Fix emergency bootloader absence before firmware update

SETUP 669 (26/04/13)
--------------------
EF_HD4(S32H3F13I11) : fix hbbTV absence on hardware H3

SETUP 668 (26/03/31)
--------------------
RM82(H3V30) : fix relock forced even when no change in dCSS config 
RM98(H1v92) : see above
RMIP(H1V58) : see above
RR12(HxV53) : see above

SETUP 667 (26/03/25)
--------------------
RM82(H3V29) : fix dCSS not sent when demodulator already locked but configuration has changed
RM98(H1v91) : see above
RMIP(H1V57) : see above
RR12(HxV52) : see above

SETUP 666 (26/03/11)
--------------------
RM82(H3V28) : CAM speed increased from 80Mpbs to 100Mbps (fix cc error on Twise CAM w/ 16 services)

SETUP 665 (26/03/11)
--------------------
RM98(H1V90) : LNBH26 - 13V output voltage increased (+ 700mV)

SETUP 664 (26/03/10)
--------------------
DTVIFACE(v384) : RM98/RMIP/RM82/RR12 : fix dCSS info in html report

SETUP 663 (26/03/06)
--------------------
RMIP(H1V56) : CAM Twise compatibility problem : ca_pmt intra splitted TPDU time reduced (AO_CI task priority increased for splitted frame) + PID without CA descriptor removed from CA_PMT

SETUP 662 (26/03/03)
--------------------
DTVIFACE(v383) : activation of services for subsequent modules allowed (cf S-bridge usage)

SETUP 661 (26/03/02)
--------------------
DTVIFACE(v382) : RMIP - IP menu cosmetics modification

SETUP 660 (26/02/24)
--------------------
RMIP(H1V55) : SID pid remapping - fix wrong SID after power-up

SETUP 659 (26/02/19)
--------------------
DTVRR14(H1V36) : watchdog TS missing w/ tuner locked : added

SETUP 658 (26/02/18)
--------------------
EF_HD4(H3V31) : Software and encoder firmware files added

SETUP 657 (26/02/17)
--------------------
EF_RM82(RM22H3 V27) : fix PAT/SDT not sent to CAM - ca_pmt intra splitted TPDU time reduced (Twise CAM incompatibility)

SETUP 656 (26/02/16)
--------------------
DTVIFACE(v381) : RM82 fix module name + Deactivation of backplane output when followed by CI module

SETUP 655 (26/01/15)
--------------------
DTVIFACE(v380) : fix cpu calibration value saving (manufacturer mode only)

SETUP 654 (26/01/12)
--------------------
DTVIFACE(v379) : Service name editable : RM98 - RM22
RM98(v89) : added Service name editable 
EF_RM22(H2/H3 V26) : added Service name editable 
EF_RR12(H2/H3-H4 V51) : added Service name editable 
RMIP(V54) : added audio dolby ac3 pid type to decryptable PID 

SETUP 653 (26/01/06)
--------------------
DTVIFACE(v378) : T2Mi management added for RM98
RM98(v88) : t2mi stream added (fpga firmware v15)

SETUP 652 (25/12/19)
--------------------
DTVIFACE(v377) : T2Mi management added in BISS settings dialog form - only RMIP
RMIP(v53) : backplane input improved - t2mi stream added (fpga firmware v15)

SETUP 651 (25/12/19)
--------------------
RMIP(v52) : stid135 driver modified - eutelsat 5 12606V stream 4 transponder correction

SETUP 650 (25/12/19)
--------------------
DTVIFACE(v376) : DTVRR12 Hardware #4 added

SETUP 649 (25/12/17)
--------------------
DTVIFACE(v375) : DTVPCU_CS : current sensing value reading modified

SETUP 648 (25/12/15)
--------------------
RR12/13(H3S49F14) : stid135 driver modified - eutelsat 5 12606V stream 4 transponder correction

SETUP 647 (25/10/24)
--------------------
EFHD4/IT9919(HW32) added IT9919-N HDCP keys programmation via EDID write command

SETUP 646 (25/10/07)
--------------------
DTVIFACE(v374) fix RM98 userband disappeared

SETUP 645 (25/10/02)
--------------------
RM98(v87) fix Twise CAM random service not descrambled (time between splitted TPDUs reduced)

SETUP 644 (25/09/15)
--------------------
DTVIFACE(v373) reboot time management added on RMIP(v51) - based on UTC time - require available time from satellite (at least one working mux)

SETUP 643 (25/09/12)
--------------------
DTVPCU(v26) current sensing management (for capable hardware)
DTVIFACE(v372) management of DTVPCU w/ current sensing management + multistream parameter hidden instead of disabled when multistream_pls_enabled unchecked

SETUP 642 (25/08/18)
--------------------
RMIP(v51) EIT filtering correction + UTC_reboot_time capability added (utc_reboot_time still to be implemented in DTVIFace)
RM98(v86) multistream_pls_enabled option added
DTVIFACE(v371) multistream_pls_enabled option for RM98 + reboot confirmation added

SETUP 641 (25/05/26)
--------------------
DTVDM4H4(v60) apply V60 to DTVMD4H4 (old hardware without Efinix) - SDT Fix

SETUP 640 (25/04/03)
--------------------
DTVIFACE(370) fix html files corrupted when using some cyrillic characters -> html file now in UTF-8 

SETUP 639 (25/03/27)
--------------------
DTVIFACE(369) fix HTML config get crash for DTVDMXITE modulators in dvbc mode

SETUP 638 (25/02/12)
--------------------
DTVIFACE(V368) : added default channel list for HD4 module (check config/channel.csv in setup directory)

SETUP 637 (25/02/07)
--------------------
DTVIFACE(V367) : added EIT_REMOVE option (get around for multiplexes with high rate EIT crash w/ RR12/13)
RR12/13(H3S47F14)

SETUP 636 (25/01/30)
--------------------
RMIP(S50H1F4) : fix server configuration problem via DTVServer (for big size configuration)

SETUP 635 (24/12/16)
--------------------
DTVIFACE(V366) : fix bug introduced in V364 - can not connect to ethernet module 

SETUP 634 (24/12/13)
--------------------
DTVIFACE(V365) : EKS verson only : dCSS/SCR default user band frequencies modified

SETUP 633 (24/11/20)
--------------------
DTVIFACE(V364) : all level now shown in dbµV - sorting function added on headends network list

SETUP 632 (24/11/15)
--------------------
RM22Hx(V25) : CAM watchog modification for Kabelio CAM (long timeout when version 1.0103 detected + cam power off/on time increased (1->2 secs))

SETUP 631 (24/10/23)
--------------------
RM98Hx(V85) : fix SID remapping bug (SID badly remapped after power-up)

SETUP 630 (24/10/22)
--------------------
RM98Hx(V84) : fix bug introduced in V83 - Abertis + previous modules streams no longer starts after power-up

SETUP 629 (24/10/16)
--------------------
RM98H3(V83) : V83 for hardware #3

SETUP 628 (24/10/14)
--------------------
RM98(V83) : detection of TP eutelsat 5 12606 before going in raw bb frame mode + fix false inactivity detection (random reboot at startup when heavy loaded TP configured)

SETUP 627 (24/10/11)
--------------------
RM98(V82) : eutelsat 5 correction removed - problem w/ eutelsat 9B

SETUP 626 (24/10/09)
--------------------
RM98(V81) : fix eutelsat 5 TP 12606MHz/stream4 can not lock

SETUP 625 (24/09/05)
--------------------
DTVIFACE(V362) : RMIP pid count displayed (instead of CPU usage) - DVB-T out freq. can now be defined from 50 to 860MHz

SETUP 624 (24/09/05)
--------------------
RMIP(S49H1F4) : pids filter use percentage added
DTVIFACE(V361) : same as above (only for RMIP)

SETUP 623 (24/08/28)
--------------------
RMIP(S48H1F4) : software reset correction - ethernet link speed auto-negociation modified + watchdog added (module not restarting after reset on some switches)

SETUP 622 (24/08/26)
--------------------
DTVIFACE(V360) : Fix EFHD4 not updated

SETUP 621 (24/08/12)
--------------------
RM98(S80H3F10) : version 80 ported to hardware #3

SETUP 620 (24/07/18)
--------------------
DTVIFACE(V359) : CAT mixing checkbox added for RMIP

SETUP 619 (24/07/16)
--------------------
EFRR14(S45H2F20) : watchdog for no output w/ input present and service activated + output bandwidth level indication
DTVIFACE(V358) : output bw indication for EF_RR1x

SETUP 618 (24/07/15) 
--------------------
RM98(S80H1F10) : new fix for bein sport 1 video errors (false PCR injection/extraction)

SETUP 617 (24/07/11) 
--------------------
EFHD4(S31H2F12Ix) : fix EFHD4 update corruption

SETUP 616 (24/06/21) 
--------------------
RM98(S78H1F9) : add LNB voltage = 0V when tuner not used by demodulators and during power up
DTVIface(V358) : communication improved on windows 11 PC (USB frame shorter + no freeze for Efinix module update)
                 EFHD4 no more updated (last version corrupted ?)

SETUP 615 (24/06/20) 
--------------------
RM98(S77H1F9) : fix CAT mixing used even when not set

SETUP 614 (24/06/18) 
--------------------
RM98(S76HxF9) : timeout added when TS over pid absent (abertis streams -> fix no output when services in grey)
DTVIface(V357) : fix bad configuration setting when click on not locked multistream/abertis service in program list  

SETUP 613 (24/06/12) 
--------------------
DTVIface(V356) : add RM82 (RM22H3) module management

SETUP 612 (24/06/10) 
--------------------
RMIP(S47H1F14) : fix adaptation field management error - false PCR detection

SETUP 611 (24/06/10) 
--------------------
RM98(S75H3F9) : fix bein sport 1 video errors (adaptation field management error - false PCR detection)

SETUP 610 (24/06/07) 
--------------------
RM98(S75H1F9) : fix bein sport 1 video errors (adaptation field management error - false PCR detection)

SETUP 609 (24/06/06) 
--------------------
IP_DVB(S26H2F14) : fix communication errors + HEVC video type recognition added

SETUP 608 (24/05/31) 
--------------------
EF_HD4(S30H2F12) : fix cc errors w/ RR1x

SETUP 607 (24/05/22) 
--------------------
DTVIface(V355) : add module selection before reset to factory default 

SETUP 606 (24/05/16) 
--------------------
RMIP-T(S46H3F11) : fix backplane input 

SETUP 605 (24/05/13) 
--------------------
EFRM22(S24H2F13) : fix SID re-allocation 

SETUP 604 (24/05/08) 
--------------------
DTVIFACE(V354) : cam watchdog added for EFRM22
EFRM22(S23H2F13) : see above

SETUP 603 (24/05/03) 
--------------------
DTVIFACE(V353) : RM22 input/demodulator configuration modified (same as RM98 -> for RM82 future compatibility)
EFRR12(S44HxF14) : watchdog added for USB hot insertion error detection

SETUP 602 (24/04/19) 
--------------------
DTVIFACE(V352)/RMIP(S46H1F13) : add dCSS/SCR LNB management for RMIP

SETUP 601 (24/03/18) 
--------------------
DTVHD4(S30H2F11) : Fix compatibility problem w/ IPDVB/DTVIPi backplane output

SETUP 600 (24/03/04) 
--------------------
DTVIface(V351) : IPDVB/DTVIPi name/type display discrimination

SETUP 599 (24/02/13) 
--------------------
RM98(V74) : avoiding service interruption on CAT change (cf. turksat mux.)

SETUP 598 (24/01/30) 
--------------------
DTVIface(V350) : other display correction when windows display parameter = 125% or 175%

SETUP 597 (24/01/29) 
--------------------
DTVIface(V349)-RMIPS45H1F13 : service decryption -> watchdog added

SETUP 596 (24/01/25) 
--------------------
DTVIface(V348) : display correction when windows display parameter = 125% or 175%

SETUP 595 (24/01/23) 
--------------------
DTVIface(V347)-DTVPCU(S25H2) : management added for redundant PSU 

SETUP 594 (24/01/10) 
--------------------
DTVIface(V345)-RMIP/IPOUT64(V44) : LG pro:idiom encryption added

SETUP 593 (23/11/22) 
--------------------
DTVRR9(S77H0F10I7) : watchdog added on HDUSB replies 
DTVIPI(S25H2F14) : SDT without service name crash fixed

SETUP 592 (23/11/20) 
--------------------
DTVIPI(S23H0F5) : SDT without service name crash fixed
DTVIface(V344) :  is_fragmented_config_capable module detection fixed (DTVIPi w/ version >= 23 detection problem)

SETUP 591 (23/11/15) 
--------------------
RMIP : Canal+ cardless CAM correction 

SETUP 590 (23/10/31) 
--------------------
RMIP : Licence key now required for DRM encryption activation

SETUP 589 (23/10/25) 
--------------------
DTVRR12/13 : macroblocks correction (problem introduced w/ FPGA v15(eit correction) - back to FPGA v14)

SETUP 588 (23/09/27) 
--------------------
DTVIface : DTVRR12 BISS menu activation correction (no BISS on recent h/w H2/H3)

SETUP 587 (23/09/20) 
--------------------
DTVHD4/DTVRR13H3 : hdcp enable/disable added (in advanced mode only)

SETUP 586 (23/09/19) 
--------------------
DTVIPi/IPDVB : backplane output clock now adjustable

SETUP 585 (23/09/18) 
--------------------
RMIP : EIT w/ scheduled events now activable or not

SETUP 584 (23/09/14) 
--------------------
. DTVIFACE : DTVIP out slots number correction (bug introduced in version 336)

SETUP 583 (23/09/14) 
--------------------
. DTVIFACE : IPDVB management added
. DTVIPiH2/IPDVB : DVBT/C modulation added - Services increased - Output bandwidth reduced to 200 Mb/s (problem with cascaded DM4F) 

SETUP 582 (23/09/06) 
--------------------
. RM98 : DOLBY_AC3_AUDIO (0x81) stream type added for audio PID detection when no audio descriptor present

SETUP 581 (23/09/04) 
--------------------
. RMIP/IP64 : audio PID filtering added

SETUP 580 (23/08/11) 
--------------------
. DTVIFACE : DTVIPI management added for hardware H2 (1Gb ethernet /  31 services)

SETUP 579 (23/07/31) 
--------------------
. DTVIface : log button now visible to all + definable logs directory path 
. RMIP : added TSID + ONID info for each stream in log (required info for some TV sets using EIT informations)

SETUP 578 (23/07/10) 
--------------------
. DTVIface : DTVAV2 management added for hardware H3

SETUP 577 (23/06/30) 
--------------------
. DTVIface + RMIP : abertis stream management added

SETUP 576 (23/06/28) 
--------------------
. DTVIface : fix RMIP random config error when following an output module

SETUP 575 (23/06/15) 
--------------------
. DTVIface : html configuration info added for DTVIP64/RMIP/RMIPT

SETUP 574 (23/06/14) 
--------------------
. DTVIface : information added on configuration load (.dtc file) mismatch

SETUP 573 (23/06/13) 
--------------------
. DTVIface : translate correction ("annuler" in config load menu)
. RMIP : EIT correction + EIT shedule added

SETUP 572 (23/05/23) 
--------------------
. DTVRR13 : remove audio pid stream from PMT when no audio present at HDMI input or in USB file (compatibily problem with some IP TVs)

SETUP 571 (23/05/05)
--------------------
. DTVIface : DTVIP64 - fix configuration error/change when followed by DVBT/C output module

SETUP 570 (23/05/03)
--------------------
. DTVIface : MHz->KHz display correction for RM98/RM22 DVBT/C Modulation

SETUP 569 (23/04/18)
--------------------
. DTVIface : added RMIP_T configuration
. RMIP/DTVIP64 : update firmware correction S35HxF7 -> S36HxF10 (bitrate overflow when TS from backplane)

SETUP 568 (23/03/30)
--------------------
. DTVIface : Added DTVRR12 bad emergency bootloader detection - user upgrade no longer allowed when detected

SETUP 567 (23/03/30)
--------------------
. RMIP/DTVIP64 : fix packets broadcasted on port 666

SETUP 566 (23/03/22)
--------------------
. DTVIface : remove HD LCN column for all OEM version + CIx added to RMIP module name

SETUP 565 (23/02/24)
--------------------
. RMIP : AES encryption : Teletext and data PIDs excluded from encryption list

SETUP 564 (23/02/23)
--------------------
. DTVIFACE : dtvserver wireless access fix (socket - fragmented packets correction)

SETUP 563 (23/02/22)
--------------------
. DTVRR10 - task scheduling modified to fix long time mux lock

SETUP 562 (23/02/15)
--------------------
. RM22 (new hardware) - CAM access correction (mutex added)
. RMIP : emergency bootloader correction

SETUP 561 (23/02/13)
--------------------
. DTVRR5 firmware V128 added
. DTVHD4 (new hardware) logs from H264 encoder deactivated

SETUP 560 (23/02/09)
--------------------
. RMIP : ip configuration got from DHCP stored in configuration (for display in DTVIface)
. DTVIface : activated service count : overflow correction + display for DTVRR12/13/14  

SETUP 559 (23/02/08)
--------------------
. DTVHD4 (old hardware) : added skybox possible power-up detection for IT9919 reset / green bar problem

SETUP 558 (23/02/07)
--------------------
. RM22 : CAT management correction (CAM TIMUCAT 5.3 blocking)
. DTVIP : max PID number by service increased

SETUP 557 (23/02/06)
--------------------
. DTVIface window resize correction (multiple monitor usage + service list width problem)

SETUP 556 (23/01/30)
--------------------
. DTVIface windows height redefinable + automatic correction of tesla.mdware.org => dtvremote.eu

SETUP 555 (23/01/25)
--------------------
. DTVIFace display correction when windows display parameters scale is not 100% and advanced parameters are activated (clear text)

SETUP 554 (23/01/23)
--------------------
. DTVHD4 (new hardware) : logs from H264 extracted

SETUP 553 (23/01/12)
--------------------
. DVBS/DVBS2 for DTVRR12H1 no more selectable : fixed

SETUP 552 (23/01/10)
--------------------
. DVB-C annex B added for DTVRR14 (new hardware)

SETUP 551 (23/01/05)
--------------------
. ethernet/internet access memory overflow correction on PC Management software

SETUP 550 (22/12/16)
--------------------
. CAT management correction on RMIP 

SETUP 549 (22/12/15)
--------------------
. add DTVIP64 backplane output ability (so that it can be followed by another output module)

SETUP 548 (22/12/12)
--------------------
. fix Cyrillic alphabet management 

SETUP 547 (22/12/08)
--------------------
. add output services count indication for RM98/RMIP/RM22 modules
. add extra EMM pids for DTVRR12/13 modules 

SETUP 546 (22/12/07)
--------------------
. fix communication problem on DTVHD4 when used with racks-5-slots on slot 3 and greater
. add ext-ci2 for RM22-H2

SETUP 545 (22/11/28)
--------------------
. add RM22 new hardware (H2) module detection

SETUP 544 (22/11/22)
--------------------
. video capture drivers of H264 ic encoder on DTVHD4 module updated (horizontal synchro problem / green bar with sky boxes)
. hsync offset removed

SETUP 543 (22/11/17)
--------------------
. fix RMIP abnormally long startup when used with ext-ci2
. add 6MHz bandwidth on DTVRR14 (new hardware) 

SETUP 542 (22/11/14)
--------------------
. user password reset allowed for OEM (when OEM password entered) 

SETUP 541 (22/11/10)
--------------------
. fix CAM menu display problem on viaccess ORCA CAM
. setup version file added in installation directory

SETUP 540 (22/11/09)
--------------------
. add dCss/scr on DTVRR12/13 (new hardware)
. modify backplane bitrate for DTVRR12/13 (new hardware) : now 300, 200, 150, 120, 100... Mb/s allowed
. fix RMIP/DTVIP64 detection problem
	
SETUP 539 (22/11/04)
--------------------
. modify backplane bitrate for DTVRR14 (new hardware) : now 300, 200, 150, 120, 100... Mb/s allowed
	
SETUP 538 (22/11/02)
--------------------
. 6MHz output bandwidth added on all modulators
. diseqc auto resent every 10 secs when no demodulator locked at all on an RF input on RM98 + DTVRR12/13 (new hardware)
	
SETUP 537 (22/10/31)
--------------------
. fix bitrate not displayed when 6MhZ output bandwidth selected on RM98
	
SETUP 536 (22/10/27)
--------------------
. agc correction in DTVRR14 (new hardware) firmware
	
SETUP 535 (22/10/11)
--------------------
. fix RAI mux problem on demodulators E-H for RM98
	
SETUP 534 (22/10/06)
--------------------
. add DTVIP64 detection
	
SETUP 533 (22/09/27)
--------------------
. detection of packet errors improved on DTVRR14 (new hardware)


   
